This page is part of a downloaded copy of this specification. This page is part of the Da Vinci Coverage Requirements Discovery (CRD) FHIR IG (v0.1.0: STU 1 Ballot 1) based on FHIR v3.5.0. . For a full list of available versions, see the Directory of published versions

This is a pre-release version (Ballot 1) of Coverage Requirements Discovery (CRD) R1/STU. There is no current official version.
For a full list of available versions, see the Directory of published versions .

## StructureDefinition: CRD Device

The official URL for this profile is:

    http://hl7.org/fhir/us/davinci-crd/StructureDefinition/profile-device-r4

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Text Summary
- Differential Table
- Snapshot Table
- All

This structure is derived from Device

Summary

Mandatory: 2 elements
Must-Support: 8 elements

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* |  |
udiCarrier | S | 1..1 | BackboneElement |
deviceIdentifier | S | 0..1 | string |
type | S | 1..1 | CodeableConcept | Binding: FHIRDeviceTypes (required)
coding | S | 0..* | Coding |
system | S | 0..1 | uri |
code | S | 0..1 | code |
property | S | 0..* | BackboneElement |
parent | S | 0..1 | Reference(Device) |
Documentation for this format

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device | I | 0..* |  | Item used in healthcare
id | Î£ | 0..1 | id | Logical id of this artifact
meta | Î£ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Î£ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: Common Languages (preferred)
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional Content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | S Î£I | 1..1 | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
deviceIdentifier | S Î£ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Î£ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Î£ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required)
status | ?!Î£ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required)
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible)
distinctIdentificationCode |  | 0..1 | string | The distinct identification code for a biological product regulated as a device
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName | I | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required)
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: FHIRDeviceTypes (required)
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | S Î£ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | S Î£ | 0..1 | uri | Identity of the terminology system
version | Î£ | 0..1 | string | Version of the system - if relevant
code | S Î£ | 0..1 | code | Symbol in syntax defined by the system
display | Î£ | 0..1 | string | Representation defined by the system
userSelected | Î£ | 0..1 | boolean | If this coding was chosen directly by the user
text | Î£ | 0..1 | string | Plain text representation of the concept
specialization | I | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version | I | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property | S I | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuanity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Î£ | 0..* | CodeableConcept | Safety Characteristics of Device
parent | S | 0..1 | Reference(Device) | The parent device
Documentation for this format

This structure is derived from Device

Summary

Mandatory: 2 elements
Must-Support: 8 elements

Differential View

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* |  |
udiCarrier | S | 1..1 | BackboneElement |
deviceIdentifier | S | 0..1 | string |
type | S | 1..1 | CodeableConcept | Binding: FHIRDeviceTypes (required)
coding | S | 0..* | Coding |
system | S | 0..1 | uri |
code | S | 0..1 | code |
property | S | 0..* | BackboneElement |
parent | S | 0..1 | Reference(Device) |
Documentation for this format

Snapshot View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device | I | 0..* |  | Item used in healthcare
id | Î£ | 0..1 | id | Logical id of this artifact
meta | Î£ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Î£ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: Common Languages (preferred)
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional Content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | S Î£I | 1..1 | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
deviceIdentifier | S Î£ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Î£ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Î£ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required)
status | ?!Î£ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required)
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible)
distinctIdentificationCode |  | 0..1 | string | The distinct identification code for a biological product regulated as a device
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName | I | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required)
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: FHIRDeviceTypes (required)
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | S Î£ | 0..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | S Î£ | 0..1 | uri | Identity of the terminology system
version | Î£ | 0..1 | string | Version of the system - if relevant
code | S Î£ | 0..1 | code | Symbol in syntax defined by the system
display | Î£ | 0..1 | string | Representation defined by the system
userSelected | Î£ | 0..1 | boolean | If this coding was chosen directly by the user
text | Î£ | 0..1 | string | Plain text representation of the concept
specialization | I | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version | I | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property | S I | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | xml:id (or equivalent in JSON)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Î£ | 0..* | Extension | Extensions that cannot be ignored if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuanity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Î£ | 0..* | CodeableConcept | Safety Characteristics of Device
parent | S | 0..1 | Reference(Device) | The parent device
Documentation for this format

Other representations of profile: Schematron

### Terminology Bindings

Path | Name | Conformance | ValueSet
Device.language | Language | preferred | Common Languages
Device.udiCarrier.entryType | UDIEntryType | required | UDIEntryType
Device.status | FHIRDeviceStatus | required | FHIRDeviceStatus
Device.statusReason | FHIRDeviceStatusReason | extensible | FHIRDeviceStatusReason
Device.deviceName.type | DeviceNameType | required | DeviceNameType
Device.type | FHIR Device Types | required | FHIRDeviceTypes

### Constraints

Id | Path | Details | Requirements
dom-2 | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources : contained.contained.empty() |
dom-4 | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated : contained.meta.versionId.empty() and contained.meta.lastUpdated.empty() |
dom-3 | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource : contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty() |
dom-6 | Device | A resource should have narrative for robust management : text.div.exists() |
dom-5 | Device | If a resource is contained in another resource, it SHALL NOT have a security label : contained.meta.security.empty() |
ele-1 | Device.udiCarrier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | Device.deviceName | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | Device.specialization | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | Device.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | Device.property | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |