This page is part of a downloaded copy of this specification. This page is part of the Da Vinci Coverage Requirements Discovery (CRD) FHIR IG (v0.1.0: STU 1 Ballot 1) based on FHIR v3.5.0. . For a full list of available versions, see the Directory of published versions

## StructureDefinition: CRD Location - Mappings

Mappings for the Profile.

### Mappings for RIM Mapping (http://hl7.org/v3)

CRD Location
Location | Entity. Role, or Act
text | Act.text?
contained | N/A
extension | N/A
modifierExtension | N/A
identifier | .id
status | .statusCode
operationalStatus | n/a
name | .name
alias | .name
description | .playingEntity[classCode=PLC determinerCode=INSTANCE].desc
mode | .playingEntity[classCode=PLC].determinerCode
type | .code
telecom | .telecom
address | .addr
id | n/a
extension | n/a
use | unique(./use)
type | unique(./use)
text | ./formatted
line | AD.part[parttype = AL]
city | AD.part[parttype = CTY]
district | AD.part[parttype = CNT | CPA]
state | AD.part[parttype = STA]
postalCode | AD.part[parttype = ZIP]
country | AD.part[parttype = CNT]
period | ./usablePeriod[type="IVL<TS>"]
physicalType | .playingEntity [classCode=PLC].code
position | .playingEntity [classCode=PLC determinerCode=INSTANCE].positionText
id | n/a
extension | n/a
modifierExtension | N/A
longitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
latitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
altitude | (RIM Opted not to map the sub-elements of GPS location, is now an OBS)
managingOrganization | .scopingEntity[classCode=ORG determinerKind=INSTANCE]
partOf | .inboundLink[typeCode=PART].source[classCode=SDLC]
hoursOfOperation | .effectiveTime
id | n/a
extension | n/a
modifierExtension | N/A
daysOfWeek | .effectiveTime
allDay | .effectiveTime
openingTime | .effectiveTime
closingTime | .effectiveTime
availabilityExceptions | n/a
endpoint | n/a

### Mappings for FiveWs Pattern (http://hl7.org/fhir/fivews)

CRD Location
Location |
identifier | FiveWs.identifier
status | FiveWs.status
operationalStatus | FiveWs.status
mode | FiveWs.class
type | FiveWs.class
physicalType | FiveWs.class